HCFeMn, FeSimn

Dear Sir/Madam,
    Kindly we would like to ask your offer for the table below:
1) FeSimn (Ferro Silico Manganese)                        300  MT                    
2) HCSiMn(High carbon ferromanganese)            200 MT   
· Your Prices (CFR) Bandar abas-Iran OR   Mersin -Turkey. 
· Validity of your offer:  15 Days.
· [bookmark: _GoBack]We can pay 5% Advance payment against Proforma Invoice through Bank to Bank Swift transfer T/T and 95% against issue of all shipping documents Copies.
· Method of filling and processing: We need the material in Moisture proof bags net weight 1.1 tons / bag.
·  After we approved the price, you will apply The MSDS sheet for all materials subject to our inquiry.

Packing: Moisture proof bags with net weight 1.1 tons / bag for (FeSiMn, HcFeMn)
Technical Offer requirements:
	FERROALLOYS %
	
	FERROALLOYS %

	Material
	C
	Mn
	Si
	s
	p
	
	Material
	SIZE
	 size %

	FeMnHC
	8 MAX
	74 MIN
	2.5 MIN
	0.015
	0.02
	0.18
	0.25
	
	FeSiHC 
	10-60 mm
	90

	FeSiMn
	2 MAX
	65 MIN
	15 MIN
	0.035
	0.03
	0.22
	0.25
	
	FeSiMn
	10-60 mm
	90

	
	
	
	
	
	
	
	
	
	C for Recarburisation
	03-05 mm
	 


Your quick response will be highly recommended
Sincerely,
Sabah Muhamad 
ceo@shatwan.net
009647501129062 OR 009647701525469 Viber ,Imo , whatsapp , telegram ,  
Skype: civilmatrix1	
wechat (wxid_ox8svm9xmyuz22), Skype: civilmatrix1
